4-Bit Digital Tube

Overview

“4-Bit Digital Tube” is the conventional name for a display capable of showing four numeric digits, where any possible digit, in turn, is composed of up to seven separate LED segments. (A decimal point potentially trailing each digit represents an eighth possible LED in that digit display.) Such low-cost, low-power numeric displays are common in microwave ovens, alarm clocks, induction cookers, automatic washing machines, and similar devices. In this experiment, you’ll program the Raspberry Pi to show the digits 0 through 9, sequentially, on the LED display.

Materials Needed

Raspberry Pi x1

Breadboard x1

4-Bit Digital Tube x1

Dupont jumper wires

Experimental Procedure

1. If you have not done so already, prepare your development system by installing the Python interpreter, RPi.GIO library, and wiringPi library as described in READ\_ME.TXT.
2. Install the 4-digit 8-segment LED display on your breadboard, and use Dupont jumper wires and resistors to connect it to your Raspberry Pi as illustrated in the Wiring Diagram below.
3. Execute the sample stored in this experiment’s subfolder.

If using C, compile and execute the C code:  
cd Code/C  
gcc 8segment\_4digit.c -o 8segment\_4digit.out –lwiringPi  
./8segment\_4digit.out

If using Python, launch the Python script:  
cd Code/Python  
python 8segment\_4digit.py

1. Make experimental observations.  
   The LED display cycles through 10 digits and the decimal point.


Product Description


Brief Introduction

Function:The digital tube is a semiconductor light emitting device whose basic unit is a light emitting diode. Therefore, series resistance is also needed to prevent excessive current.

Application: Digital tube is widely used in instruments, clocks, stations, etc.

Pin description:






Parameters

◆ Model: common anode

◆ Size: length 30mm\* width 14mm\* thickness 7.2mm

◆ lighting color: bright red

Wiring diagram



Sample Code

1. Python code

#!/usr/bin/env python

import RPi.GPIO as GPIO

import time

pins = {'pinA':3, 'pinB':5, 'pinC':21, 'pinD':8, 'pinE':10, 'pinF':11, 'pinG':12, 'pinDP':13, 'pin\_1':15, 'pin\_2':16, 'pin\_3':18, 'pin\_4':19}

def init():

GPIO.setmode(GPIO.BOARD)

for i in pins:

GPIO.setup(pins[i], GPIO.OUT)

print 'gpio init completed!'

def bitSelect(bitNum):

if(bitNum == 1):

GPIO.output(pins['pin\_1'], GPIO.HIGH)

GPIO.output(pins['pin\_2'], GPIO.LOW)

GPIO.output(pins['pin\_3'], GPIO.LOW)

GPIO.output(pins['pin\_4'], GPIO.LOW)

elif(bitNum == 2):

GPIO.output(pins['pin\_1'], GPIO.LOW)

GPIO.output(pins['pin\_2'], GPIO.HIGH)

GPIO.output(pins['pin\_3'], GPIO.LOW)

GPIO.output(pins['pin\_4'], GPIO.LOW)

elif(bitNum == 3):

GPIO.output(pins['pin\_1'], GPIO.LOW)

GPIO.output(pins['pin\_2'], GPIO.LOW)

GPIO.output(pins['pin\_3'], GPIO.HIGH)

GPIO.output(pins['pin\_4'], GPIO.LOW)

elif(bitNum == 4):

GPIO.output(pins['pin\_1'], GPIO.LOW)

GPIO.output(pins['pin\_2'], GPIO.LOW)

GPIO.output(pins['pin\_3'], GPIO.LOW)

GPIO.output(pins['pin\_4'], GPIO.HIGH)

else:

GPIO.output(pins['pin\_1'], GPIO.LOW)

GPIO.output(pins['pin\_2'], GPIO.LOW)

GPIO.output(pins['pin\_3'], GPIO.LOW)

GPIO.output(pins['pin\_4'], GPIO.LOW)

print 'bitSelect completed!'

def display\_0():

GPIO.output(pins['pinA'], GPIO.LOW)

GPIO.output(pins['pinB'], GPIO.LOW)

GPIO.output(pins['pinC'], GPIO.LOW)

GPIO.output(pins['pinD'], GPIO.LOW)

GPIO.output(pins['pinE'], GPIO.LOW)

GPIO.output(pins['pinF'], GPIO.LOW)

GPIO.output(pins['pinG'], GPIO.HIGH)

GPIO.output(pins['pinDP'], GPIO.HIGH)

print 'display number 0'

def display\_1():

GPIO.output(pins['pinA'], GPIO.HIGH)

GPIO.output(pins['pinB'], GPIO.LOW)

GPIO.output(pins['pinC'], GPIO.LOW)

GPIO.output(pins['pinD'], GPIO.HIGH)

GPIO.output(pins['pinE'], GPIO.HIGH)

GPIO.output(pins['pinF'], GPIO.HIGH)

GPIO.output(pins['pinG'], GPIO.HIGH)

GPIO.output(pins['pinDP'], GPIO.HIGH)

print 'display number 1'

def display\_2():

GPIO.output(pins['pinA'], GPIO.LOW)

GPIO.output(pins['pinB'], GPIO.LOW)

GPIO.output(pins['pinC'], GPIO.HIGH)

GPIO.output(pins['pinD'], GPIO.LOW)

GPIO.output(pins['pinE'], GPIO.LOW)

GPIO.output(pins['pinF'], GPIO.HIGH)

GPIO.output(pins['pinG'], GPIO.LOW)

GPIO.output(pins['pinDP'], GPIO.HIGH)

print 'display number 2'

def display\_3():

GPIO.output(pins['pinA'], GPIO.LOW)

GPIO.output(pins['pinB'], GPIO.LOW)

GPIO.output(pins['pinC'], GPIO.LOW)

GPIO.output(pins['pinD'], GPIO.LOW)

GPIO.output(pins['pinE'], GPIO.HIGH)

GPIO.output(pins['pinF'], GPIO.HIGH)

GPIO.output(pins['pinG'], GPIO.LOW)

GPIO.output(pins['pinDP'], GPIO.HIGH)

print 'display number 3'

def display\_4():

GPIO.output(pins['pinA'], GPIO.HIGH)

GPIO.output(pins['pinB'], GPIO.LOW)

GPIO.output(pins['pinC'], GPIO.LOW)

GPIO.output(pins['pinD'], GPIO.HIGH)

GPIO.output(pins['pinE'], GPIO.HIGH)

GPIO.output(pins['pinF'], GPIO.LOW)

GPIO.output(pins['pinG'], GPIO.LOW)

GPIO.output(pins['pinDP'], GPIO.HIGH)

print 'display number 4'

def display\_5():

GPIO.output(pins['pinA'], GPIO.LOW)

GPIO.output(pins['pinB'], GPIO.HIGH)

GPIO.output(pins['pinC'], GPIO.LOW)

GPIO.output(pins['pinD'], GPIO.LOW)

GPIO.output(pins['pinE'], GPIO.HIGH)

GPIO.output(pins['pinF'], GPIO.LOW)

GPIO.output(pins['pinG'], GPIO.LOW)

GPIO.output(pins['pinDP'], GPIO.HIGH)

print 'display number 5'

def display\_6():

GPIO.output(pins['pinA'], GPIO.LOW)

GPIO.output(pins['pinB'], GPIO.HIGH)

GPIO.output(pins['pinC'], GPIO.LOW)

GPIO.output(pins['pinD'], GPIO.LOW)

GPIO.output(pins['pinE'], GPIO.LOW)

GPIO.output(pins['pinF'], GPIO.LOW)

GPIO.output(pins['pinG'], GPIO.LOW)

GPIO.output(pins['pinDP'], GPIO.HIGH)

print 'display number 6'

def display\_7():

GPIO.output(pins['pinA'], GPIO.LOW)

GPIO.output(pins['pinB'], GPIO.LOW)

GPIO.output(pins['pinC'], GPIO.LOW)

GPIO.output(pins['pinD'], GPIO.HIGH)

GPIO.output(pins['pinE'], GPIO.HIGH)

GPIO.output(pins['pinF'], GPIO.HIGH)

GPIO.output(pins['pinG'], GPIO.HIGH)

GPIO.output(pins['pinDP'], GPIO.HIGH)

print 'display number 7'

def display\_8():

GPIO.output(pins['pinA'], GPIO.LOW)

GPIO.output(pins['pinB'], GPIO.LOW)

GPIO.output(pins['pinC'], GPIO.LOW)

GPIO.output(pins['pinD'], GPIO.LOW)

GPIO.output(pins['pinE'], GPIO.LOW)

GPIO.output(pins['pinF'], GPIO.LOW)

GPIO.output(pins['pinG'], GPIO.LOW)

GPIO.output(pins['pinDP'], GPIO.HIGH)

print 'display number 8'

def display\_9():

GPIO.output(pins['pinA'], GPIO.LOW)

GPIO.output(pins['pinB'], GPIO.LOW)

GPIO.output(pins['pinC'], GPIO.LOW)

GPIO.output(pins['pinD'], GPIO.LOW)

GPIO.output(pins['pinE'], GPIO.HIGH)

GPIO.output(pins['pinF'], GPIO.LOW)

GPIO.output(pins['pinG'], GPIO.LOW)

GPIO.output(pins['pinDP'], GPIO.HIGH)

print 'display number 9'

def display\_dp():

GPIO.output(pins['pinA'], GPIO.HIGH)

GPIO.output(pins['pinB'], GPIO.HIGH)

GPIO.output(pins['pinC'], GPIO.HIGH)

GPIO.output(pins['pinD'], GPIO.HIGH)

GPIO.output(pins['pinE'], GPIO.HIGH)

GPIO.output(pins['pinF'], GPIO.HIGH)

GPIO.output(pins['pinG'], GPIO.HIGH)

GPIO.output(pins['pinDP'], GPIO.LOW)

print 'display DP'

def clear(): #clear the screen

GPIO.output(pins['pinA'], GPIO.HIGH)

GPIO.output(pins['pinB'], GPIO.HIGH)

GPIO.output(pins['pinC'], GPIO.HIGH)

GPIO.output(pins['pinD'], GPIO.HIGH)

GPIO.output(pins['pinE'], GPIO.HIGH)

GPIO.output(pins['pinF'], GPIO.HIGH)

GPIO.output(pins['pinG'], GPIO.HIGH)

GPIO.output(pins['pinDP'], GPIO.HIGH)

print 'clear the screen!'

def pickNum(number):

if(number == 0):

display\_0()

elif(number == 1):

display\_1()

elif(number == 2):

display\_2()

elif(number == 3):

display\_3()

elif(number == 4):

display\_4()

elif(number == 5):

display\_5()

elif(number == 6):

display\_6()

elif(number == 7):

display\_7()

elif(number == 8):

display\_8()

elif(number == 9):

display\_9()

else:

clear()

def Display(Bit, Number):

bitSelect(Bit)

pickNum(Number)

time.sleep(0.001)

def loop():

while True:

Display(1,1)

time.sleep(1)

Display(2,2)

time.sleep(1)

Display(3,3)

time.sleep(1)

Display(4,4)

time.sleep(1)

if \_\_name\_\_ == '\_\_main\_\_':

try:

init()

loop()

except KeyboardInterrupt:

GPIO.cleanup()

print 'Key Board Interrupt!'

2. C Code

#include <wiringPi.h>

#include <stdio.h>

//display 1234

//Set cathode interface

int a = 8;

int b = 9;

int c = 13;

int d = 15;

int e = 16;

int f = 0;

int g = 1;

int dp = 2;

//Set anode interface

int d4 = 12;

int d3 = 5;

int d2 = 4;

int d1 = 3;

//Set variable

long n = 1230;

int x = 100;

int del = 55; //Here to fine tune the clock

void init()

{

pinMode(d1, OUTPUT);

pinMode(d2, OUTPUT);

pinMode(d3, OUTPUT);

pinMode(d4, OUTPUT);

pinMode(a, OUTPUT);

pinMode(b, OUTPUT);

pinMode(c, OUTPUT);

pinMode(d, OUTPUT);

pinMode(e, OUTPUT);

pinMode(f, OUTPUT);

pinMode(g, OUTPUT);

pinMode(dp, OUTPUT);

}

void bitSelect(unsigned char n)//

{

switch(n)

{

case 1:

digitalWrite(d1,HIGH);

digitalWrite(d2, LOW);

digitalWrite(d3, LOW);

digitalWrite(d4, LOW);

break;

case 2:

digitalWrite(d1, LOW);

digitalWrite(d2, HIGH);

digitalWrite(d3, LOW);

digitalWrite(d4, LOW);

break;

case 3:

digitalWrite(d1,LOW);

digitalWrite(d2, LOW);

digitalWrite(d3, HIGH);

digitalWrite(d4, LOW);

break;

case 4:

digitalWrite(d1, LOW);

digitalWrite(d2, LOW);

digitalWrite(d3, LOW);

digitalWrite(d4, HIGH);

break;

default :

digitalWrite(d1, LOW);

digitalWrite(d2, LOW);

digitalWrite(d3, LOW);

digitalWrite(d4, LOW);

break;

}

}

void Num\_0()

{

digitalWrite(a, LOW);

digitalWrite(b, LOW);

digitalWrite(c, LOW);

digitalWrite(d, LOW);

digitalWrite(e, LOW);

digitalWrite(f, LOW);

digitalWrite(g, HIGH);

digitalWrite(dp,HIGH);

}

void Num\_1()

{

digitalWrite(a, HIGH);

digitalWrite(b, LOW);

digitalWrite(c, LOW);

digitalWrite(d, HIGH);

digitalWrite(e, HIGH);

digitalWrite(f, HIGH);

digitalWrite(g, HIGH);

digitalWrite(dp,HIGH);

}

void Num\_2()

{

digitalWrite(a, LOW);

digitalWrite(b, LOW);

digitalWrite(c, HIGH);

digitalWrite(d, LOW);

digitalWrite(e, LOW);

digitalWrite(f, HIGH);

digitalWrite(g, LOW);

digitalWrite(dp,HIGH);

}

void Num\_3()

{

digitalWrite(a, LOW);

digitalWrite(b, LOW);

digitalWrite(c, LOW);

digitalWrite(d, LOW);

digitalWrite(e, HIGH);

digitalWrite(f, HIGH);

digitalWrite(g, LOW);

digitalWrite(dp,HIGH);

}

void Num\_4()

{

digitalWrite(a, HIGH);

digitalWrite(b, LOW);

digitalWrite(c, LOW);

digitalWrite(d, HIGH);

digitalWrite(e, HIGH);

digitalWrite(f, LOW);

digitalWrite(g, LOW);

digitalWrite(dp,HIGH);

}

void Num\_5()

{

digitalWrite(a, LOW);

digitalWrite(b, HIGH);

digitalWrite(c, LOW);

digitalWrite(d, LOW);

digitalWrite(e, HIGH);

digitalWrite(f, LOW);

digitalWrite(g, LOW);

digitalWrite(dp,HIGH);

}

void Num\_6()

{

digitalWrite(a, LOW);

digitalWrite(b, HIGH);

digitalWrite(c, LOW);

digitalWrite(d, LOW);

digitalWrite(e, LOW);

digitalWrite(f, LOW);

digitalWrite(g, LOW);

digitalWrite(dp,HIGH);

}

void Num\_7()

{

digitalWrite(a, LOW);

digitalWrite(b, LOW);

digitalWrite(c, LOW);

digitalWrite(d, HIGH);

digitalWrite(e, HIGH);

digitalWrite(f, HIGH);

digitalWrite(g, HIGH);

digitalWrite(dp,HIGH);

}

void Num\_8()

{

digitalWrite(a, LOW);

digitalWrite(b, LOW);

digitalWrite(c, LOW);

digitalWrite(d, LOW);

digitalWrite(e, LOW);

digitalWrite(f, LOW);

digitalWrite(g, LOW);

digitalWrite(dp,HIGH);

}

void Num\_9()

{

digitalWrite(a, LOW);

digitalWrite(b, LOW);

digitalWrite(c, LOW);

digitalWrite(d, LOW);

digitalWrite(e, HIGH);

digitalWrite(f, LOW);

digitalWrite(g, LOW);

digitalWrite(dp,HIGH);

}

void Clear() // Clear the screen

{

digitalWrite(a, HIGH);

digitalWrite(b, HIGH);

digitalWrite(c, HIGH);

digitalWrite(d, HIGH);

digitalWrite(e, HIGH);

digitalWrite(f, HIGH);

digitalWrite(g, HIGH);

digitalWrite(dp,HIGH);

}

void pickNumber(unsigned char n)//Choose the number of

{

switch(n)

{

case 0:Num\_0();

break;

case 1:Num\_1();

break;

case 2:Num\_2();

break;

case 3:Num\_3();

break;

case 4:Num\_4();

break;

case 5:Num\_5();

break;

case 6:Num\_6();

break;

case 7:Num\_7();

break;

case 8:Num\_8();

break;

case 9:Num\_9();

break;

default:Clear();

break;

}

}

void Display(unsigned char x, unsigned char Number)//Show that x is the coordinate, Number is the number

{

bitSelect(x);

pickNumber(Number);

delay(1);

//Clear() ; //Vanishing

}

int main(void)

{

if(wiringPiSetup() == -1)

{

printf("wiringPi setup failed!\n");

return -1;

}

init();

while(1)

{

Display(1, 1);

delay(1000);

Display(2, 2);

delay(1000);

Display(3, 3);

delay(1000);

Display(4, 4);

delay(1000);

}

}

Experimental Phenomena

The four-bit digital tube shows the number 1234 in crycle.